**INTENSIVE CARE BEDS**

* Electric bed,
* Rechargeable battery
* 4 twin wheels, antistatic and lockable
* positions: trendelenburg, anti-trendelenburg, cardiology chair,
* electrically and mechanically achievement of PCR emergency position
* variable height, between about 40 and 80 cm at least
* extendable length
* removable headboard and footboard without sharp edges
* integrated bathroom scale
* safe working load over 220 kg
* the whole structure must have smooth, easily sanitized and resistant to corrosive agents
* Large radiolucent area for RX exams
* control panel and keyboard easily sanitized and impact resistant
* safety and alarm devices
* oxygen cylinder housing
* Support for urine bag and drainage
* Anti-decubitus mattress
* preferably compliant with the Italian medical devices legislation in force in Italy applied to medical devices.
* Supply: 220 V, 50 Hz