**MONITOR**

* Minimun size 12"
* Required signals: ECG 3/5 leads, SpO2, EtCo2 mainstream, minimum 2 Invasive pressures, NIBP;
* Visual and audible alarms,
* complete with all the necessary cables and sensors,
* preferably compliant with the Italian medical devices legislation in force in Italy applied to medical devices.
* Supply: 220 V, 50 Hz